<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0.1" y1="0.1" x2="41.1" y2="0.1" width="0" layer="20"/>
<wire x1="41.1" y1="0.1" x2="41.1" y2="39.89" width="0" layer="20"/>
<wire x1="41.1" y1="39.89" x2="0.1" y2="39.89" width="0" layer="20"/>
<wire x1="0.1" y1="39.89" x2="0.1" y2="0.1" width="0" layer="20"/>
<text>OUT</text>
<text>IN</text>
<text>IN</text>
<text>ADJ</text>
<text>OUT</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>IN</text>
<text>IN</text>
<text>B</text>
<text>C</text>
<text>E</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>8</text>
<text>1</text>
<text>4</text>
<text>5</text>
<text>7</text>
<text>6</text>
<text>2</text>
<text>3</text>
<text>NO</text>
<text>NO</text>
<text>NO</text>
<text>NO</text>
<text>IN</text>
</plain>
<libraries>
<library name="#PaJa_31">
<description>&lt;B&gt;PaJa 31&lt;/B&gt; - knihovna   &amp;nbsp; &amp;nbsp; &amp;nbsp; &amp;nbsp; &amp;nbsp; &amp;nbsp; 
&lt;I&gt;(vytvoreno 1.1.2014)&lt;/I&gt;&lt;BR&gt;
Univerzální knihovna soucastek do Eagle &lt;I&gt;(od verze 5.6)&lt;/I&gt;&lt;BR&gt;
&lt;BR&gt;
Knihovna obsahuje: 215 soucastek na DPS, 330 do SCHematu&lt;BR&gt;
&lt;BR&gt;
&lt;Author&gt;Copyright (C) PaJa 2001-2014&lt;BR&gt;
www.paja-trb.cz&lt;BR&gt;
paja@paja-trb.cz
&lt;/author&gt;</description>
<packages>
<package name="1206">
<description>&lt;B&gt;SMD&lt;/B&gt; - velikost 1206</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;SMD tranzistor&lt;/b&gt;</description>
</package>
<package name="DPAK">
<description>3-lead &lt;b&gt;SMD PACKAGE&lt;/b&gt;</description>
</package>
<package name="SOD-80">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="PANASONIC_B">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package B&lt;/b&gt;</description>
</package>
<package name="RTRIM4G/J">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; VISHAY</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
<package name="RTRIM5W">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; Spectrol&lt;p&gt;
abgedichtet nach &lt;b&gt;IP67&lt;/b&gt;</description>
</package>
<package name="L3225M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
</packages>
</library>
<library name="lm-337 smd">
<packages>
<package name="SO08">
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SE14">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.4 mm</description>
</package>
</packages>
</library>
<library name="smd-">
<description>&lt;b&gt;IPC Standard SMD Packages&lt;/b&gt;&lt;p&gt;
This is a package-only library, based on the Surface Mount Design and Land Pattern Standard developed by the 
Institute for Interconnecting and Packaging electronic Circuits (IPC).&lt;p&gt;
Source:&lt;p&gt;
IPC-SM-782&lt;br&gt;
Revision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CT3216">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C13" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="PANASONIC_B" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="#PaJa_31" package="SOT-23" value="BC848">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R7" library="#PaJa_31" package="1206" value="1M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="#PaJa_31" package="1206" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="rcl" package="RTRIM4G/J" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="#PaJa_31" package="1206" value="M1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="#PaJa_31" package="1206" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="#PaJa_31" package="1206" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="#PaJa_31" package="1206" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="#PaJa_31" package="1206" value="1K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="PANASONIC_B" value="10/16">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="#PaJa_31" package="1206" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="#PaJa_31" package="1206" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="#PaJa_31" package="1206" value="8k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="#PaJa_31" package="1206" value="1k8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="SO08" value="LM1458D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="maxim" package="SO08" value="ICL7660">
<attribute name="OC_NEWARK" value="34C3732"/>
<attribute name="MPN" value="ICL7660CSA"/>
<attribute name="MF" value="MAXIM"/>
<attribute name="OC_FARNELL" value="9724710"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IO1" library="#PaJa_31" package="DPAK" value="7805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="#PaJa_31" package="SOD-80" value="1N4148.">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C14" library="#PaJa_31" package="1206" value="100p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="PANASONIC_B" value="2,2µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="PANASONIC_D" value="100µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IO3" library="lm-337 smd" package="SO08" value="LM337">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP" library="solpad" package="SE14" value="SE14">
<attribute name="NAME"/>
</element>
<element name="IN" library="solpad" package="SE14" value="SE14">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+12V" library="solpad" package="SE14" value="+12V">
<attribute name="NAME"/>
</element>
<element name="R1" library="rcl" package="RTRIM5W" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="SO08" value="78L10SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L3225M" value="10µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="#PaJa_31" package="1206" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="smd-" package="CT3216" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="smd-" package="CT3216" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$51">
<contactref element="Q6" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="IC1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$30">
<contactref element="IC3" pad="4"/>
<contactref element="C10" pad="-"/>
</signal>
<signal name="N$27">
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="-"/>
<contactref element="IC3" pad="5"/>
<contactref element="IO3" pad="2"/>
<contactref element="IO3" pad="3"/>
<contactref element="IO3" pad="6"/>
<contactref element="IO3" pad="7"/>
</signal>
<signal name="N$42">
<contactref element="IC3" pad="8"/>
<contactref element="IO1" pad="3"/>
<contactref element="C11" pad="+"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="-"/>
<contactref element="IO3" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="R9" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q6" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IC3" pad="2"/>
<contactref element="C10" pad="+"/>
</signal>
<signal name="N$5">
<contactref element="R8" pad="2"/>
<contactref element="IN" pad="MP"/>
</signal>
<signal name="S$5">
<contactref element="IO1" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="1"/>
<contactref element="C18" pad="+"/>
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$3">
<contactref element="L1" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="L1" pad="1"/>
<contactref element="+12V" pad="MP"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="5"/>
<contactref element="C6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="N$9">
<contactref element="IO3" pad="4"/>
<contactref element="R1" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="MP" pad="MP"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="S$1">
<contactref element="P1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
